IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2018-02-14T16:01:53"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20161004_0715(x64) - Exporter 16.0.1185.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "agulsev" of Organization (no name given)
  Owner history of Person "agulsev" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1518618942 (2018-02-14T14:35:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "P:\schönox\002554 package wanden\04 package\14-02-2018\Sika Deutschland Gmbh – SCHÖNOX_R2016.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Itannex almelo"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 32 elements
          1 x IFCANNOTATION
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages_1:LOD200:87603" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX:88090" | material: layers "Floor:NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88113" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88122" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88131" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88140" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX:59304" | names: "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX:88141" | material: layers "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX:88146" | material: layers "Floor:NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX:68074" | names: "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX:88153" | material: layers "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88164" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88173" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX:88176" | material: layers "Floor:NLRS_43_FL_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX:69910" | names: "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX:88183" | material: layers "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Sporthal (Tegeltechniek)_SCHÖNOX_ITX:88189" | material: layers "Floor:NLRS_43_FL_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88203" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88212" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX:70964" | names: "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX:88213" | material: layers "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX:88219" | material: layers "Floor:NLRS_43_FL_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2., "NLRS_r4_2-componentige mortel_SCHÖNOX 2K DS RAPID afdichtingmortel_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX PL PLUS Cementgebonden egaliseermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88233" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88242" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX:72667" | names: "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX:88243" | material: layers "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX:88249" | material: layers "Floor:NLRS_43_FL_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2., "NLRS_r4_2-componenten-polyurethaan_SCHÖNOX EA PUR S Afdichtingslijm_ITX" 1., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH FIX Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88263" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88272" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX:75448" | names: "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX:88273" | material: layers "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX:88279" | material: layers "Floor:NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2., "NLRS_r4_2-componentige mortel_SCHÖNOX 2K DS RAPID afdichtingmortel_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX PL PLUS Cementgebonden egaliseermortel_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX KH Kunsthars hechtdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88293" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX" | FLOOR | names: "Floor:NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX:88297" | material: layers "Floor:NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX" ("NLRS_q2_dispersielijm_ SCHÖNOX LINOTEX Dispersielijm_ITX" 2., "NLRS_q2_Alpha-Halfhydraatbasis_SCHÖNOX AM egaliseer- en nivelleermassa_ITX" 2., "NLRS_r4_kunsthars dispersie_SCHÖNOX VD FIX Verzepingsresistente kunstharsdispersie_ITX" 1.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88311" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LOD200" | object type "LOD200" | names: "000_00_ISR_lod_packages:LOD200:88320" | material: "00_blauw" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX" | object type "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX:77116" | names: "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX:88321" | material: layers "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural

Types
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 30 FLEX Uitvlak- en pleistermortel_ITX" 2., "NLRS_q2_cementgebonden lijm, SCHÖNOX Q6 Cementgebonden poeder-tegellijm_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2., "NLRS_r4_2-componenten epoxyhars_SCHÖNOX CF DESIGN Gekleurde epoxyharsvoeg_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "LOD200" | 1 occurrence | material: "00_blauw" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX" ("NLRS_correctielaag_ITX" 1., "NLRS_q2_cementgebonden mortel_SCHÖNOX BM 10 Uitvlak- en pleistermortel_ITX" 2.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other

Property sets
  Other | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "000_00_ISR_lod_packages: LOD200" (IFCLABEL)
    Family and Type = "000_00_ISR_lod_packages: LOD200" (IFCLABEL)
    Type = "000_00_ISR_lod_packages: LOD200" (IFCLABEL)
    Type Id = "000_00_ISR_lod_packages: LOD200" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "000_00_ISR_lod_packages_1: LOD200" (IFCLABEL)
    Family and Type = "000_00_ISR_lod_packages_1: LOD200" (IFCLABEL)
    Type = "000_00_ISR_lod_packages_1: LOD200" (IFCLABEL)
    Type Id = "000_00_ISR_lod_packages_1: LOD200" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Family and Type = "Floor: NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type = "Floor: NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type Id = "Floor: NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type = "Basic Wall: NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Family and Type = "Floor: NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type = "Floor: NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
    Type Id = "Floor: NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCLABEL)
  Other: 16 more contents on 13 objects not shown
  Identity Data | properties | on 9 objects (5 IFCBUILDINGELEMENTPROXY, 4 IFCSLAB)
    Design Option = "Main Model" (IFCTEXT)
  Identity Data | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    Comments = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Comments = "" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Building Name = "" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "43.21" (IFCTEXT)
    Assembly Description = "vloerafwerkingen; niet verhoogd, afwerklagen" (IFCTEXT)
    Datum_Gewijzigd = "" (IFCTEXT)
    Description = "NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX" (IFCTEXT)
    Manufacturer = "Sika Deutschland GmbH – SCHÖNOX" (IFCTEXT)
    Model = "LOD400" (IFCTEXT)
    SmartRevit_Versie = "2016.3" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX" (IFCTEXT)
    URL = "https://www.schonox.com/nl/vloerenleggers-vloertechniek/" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Design Option = "Option Set 1 : Option 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "43.21" (IFCTEXT)
    Assembly Description = "vloerafwerkingen; niet verhoogd, afwerklagen" (IFCTEXT)
    Datum_Gewijzigd = "" (IFCTEXT)
    Description = "NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX" (IFCTEXT)
    Manufacturer = "Sika Deutschland GmbH – SCHÖNOX" (IFCTEXT)
    Model = "LOD400" (IFCTEXT)
    SmartRevit_Versie = "2016.3" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX" (IFCTEXT)
    URL = "https://www.schonox.com/nl/buiten-terras-tegeltechniek/" (IFCTEXT)
  Identity Data: 15 more contents on 7 objects not shown
  Graphics | properties | on 8 objects (8 IFCSLAB)
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 7 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Constraints | properties | on 16 objects (16 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 8 objects (8 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Core Face: Exterior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 5 objects (5 IFCSLAB)
    Default Thickness = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 2 objects (2 IFCSLAB)
    Default Thickness = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 4. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 5 type objects
    Function = "Interior" (IFCIDENTIFIER)
    Width = 4.99999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 3. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 16 objects (16 IFCBUILDINGELEMENTPROXY)
    Reference = "LOD200" (IFCIDENTIFIER)
  Dimensions | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Area = 2.99999999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0149999999999966 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 3 objects (3 IFCSLAB)
    Area = 9.00000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = -5. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 12000. (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0450000000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCSLAB)
    Area = 8.99999999999997 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = -5. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 12000. (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0449999999999998 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 27.5292011950084 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.304468084350109 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 8.02417104094628 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.157782601619971 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 8.00199133033292 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.157282798845976 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 10.0389835773168 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.197233360161363 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 10.0168038667034 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.196733557387368 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 16 more contents on 16 objects not shown
  Phasing | properties | on 31 objects (16 IFCBUILDINGELEMENTPROXY, 8 IFCSLAB, 7 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "Sika Deutschland Gmbh – SCHÖNOX vloer- en wandsystemen" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "VLOEREN: Nieuwbouw en renovatie (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "WANDEN: Nieuwbouw en renovatie (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "VLOEREN: Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "WANDEN: Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "VLOEREN: Woonstichting (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "WANDEN: Woonstichting (Tegeltechniek)" (IFCTEXT)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    benaming_package = "VLOEREN: Sporthal (Tegeltechniek)" (IFCTEXT)
  Text: 8 more contents on 8 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Buiten terras (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "NLRS_43_FL_Vloerenleggers (Vloertechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 15 objects (8 IFCSLAB, 7 IFCWALLSTANDARDCASE)
    Manufacturer = "Sika Deutschland GmbH – SCHÖNOX" (IFCLABEL)
  Structural | properties | on 8 objects (8 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Exterior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Interior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = "Bearing" (IFCIDENTIFIER)
  Analytical Properties | properties | on 8 objects (8 IFCSLAB) | on 7 type objects
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Utiliteitsbouw (geen vochtbelasting) (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Nieuwbouw en Renovatie (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Woonstichting (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Sporthal (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Zwembad algemeen (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Zwembad zoutwaterbaden (Tegeltechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "NLRS_42_WA_Stucadoorswerk (Wandtechniek)_SCHÖNOX_ITX" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "NLRS_correctielaag_ITX" (IFCLABEL)